{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Flows","Oil Change Intervals","T100 Oil Change","Torque","MotorInverter Approx KW"],"not_rendered":{"charts":2,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Flows","index":0,"n_rows":114,"n_cols":23,"rows_kept":114,"cut":false,"hidden":false,"merged":[[73,22,94,26],[88,0,94,0],[59,0,65,0],[67,0,70,0],[5,3,6,3],[44,22,70,26],[5,4,6,4],[5,5,6,5],[5,13,6,13],[5,6,6,6],[5,10,6,10],[5,0,6,0],[2,8,2,10],[113,1,114,13],[31,4,34,4],[113,0,114,0],[5,18,6,18],[4,8,4,13],[73,0,86,0],[7,0,42,0],[44,0,57,0],[96,0,102,0],[104,0,110,0],[111,0,112,0],[96,22,112,26],[1,22,4,26],[20,1,21,1],[5,11,6,11],[8,22,38,26],[5,1,6,1],[5,2,6,2],[5,17,6,17],[7,1,11,1],[13,1,17,1],[23,1,26,1],[31,1,34,1],[36,1,39,1],[1,12,1,13],[2,12,2,13],[1,8,1,10]]}
[null,null,null,null,null,null,null,null,null,{"$f":"$I$1/60","v":0},{"$f":"$J$1/$D$1","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,"Enter Discharge Pressure here (bar)",null,null,10,"for kW calculation",null,null,null,null,null,null,null,null,null,"All input is done in the yellow boxes                                                                                1. Input the maximum discharge pressure in cell K2             2. Input the required flow rate in column H and then the chosen row for the pump and CAM choice."]
[null,null,null,null,null,null,null,null,"Enter Temperature here (°C)",null,null,0,"for oil change calculation"]
[null,null,null,null,null,null,null,null,"Absorbed Power, before Transmission Losses"]
[null,null,null,null,null,null,null,null,"Flows @ 60 bar unless otherwise stated"]
[null,"Pump","Cam","Litre/Rev","@ 1450 rpm","@ 960 rpm","@ 730 rpm","Req'd Flow","Req'd Flow","Req'd Flow","RPM","Power kW @ SG=1","Oil Change Interval","Torque Req. Nm","Service Factor","Slope","Intercept","Motor Base Speed RPM","Motor Power Req'd","Forced Vent Req'd?","Encoder Req'd?","Realistic Application?"]
[null,null,null,null,null,null,null,"m3/hr","litres/hr","litres/min",null,null,"hours"]
[null,"G20 / G21 / G22","X",{"$f":"E8/1450","v":2.1655172413793103E-3},3.14,{"$f":"D8*960","v":2.0788965517241378},{"$f":"D8*730","v":1.5808275862068966},0,{"$f":"$H$8*1000","v":0},{"$f":"$I$8/60","v":0},{"$f":"$J$8/$D$8","v":0},{"$f":"($L$2*0.122495179*K8/9550)","v":0},{"$f":"IF(K8>10,IF((P8*O8)+Q8>1000,IF($L$3<100,(P8*O8)+Q8,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L8*9550/K8,\"-\")","v":"-"},{"$f":"(K8*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,1450,{"$f":"($L$2*0.122495179*R8/9550)","v":0.18598744455497382},{"$f":"IF(K8<(R8/2),TRUE,FALSE)","v":true},{"$f":"IF(K8<R8/10,TRUE,FALSE)","v":true},{"$f":"IF(K8<R8/50,FALSE,TRUE)","v":false}]
[null,null,"E",{"$f":"E9/1450","v":1.5793103448275862E-3},2.29,{"$f":"D9*960","v":1.5161379310344827},{"$f":"D9*730","v":1.1528965517241379},0,{"$f":"$H$9*1000","v":0},{"$f":"$I$9/60","v":0},{"$f":"$J$9/$D$9","v":0},{"$f":"($L$2*0.0911364131975407*K9/9550)","v":0},{"$f":"IF(K9>10,IF((P9*O9)+Q9>1000,IF($L$3<100,(P9*O9)+Q9,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L9*9550/K9,\"-\")","v":"-"},{"$f":"(K9*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"($L$2*0.0911364131975407*R9/9550)","v":0},null,null,null,"Very Important Note                                                                                                                                                                                                                                   The value given for the KW absorbed power is for the pump not the motor.                             In selecting the right motor you must check the motor data sheet and make sure that the motor chosen will give the power at the specific RPM  "]
[null,null,"S",{"$f":"E10/1450","v":1.1862068965517241E-3},1.72,{"$f":"D10*960","v":1.1387586206896552},{"$f":"D10*730","v":0.86593103448275865},0,{"$f":"$H$10*1000","v":0},{"$f":"$I$10/60","v":0},{"$f":"$J$10/$D$10","v":0},{"$f":"($L$2*0.0734971074173716*K10/9550)","v":0},{"$f":"IF(K10>10,IF((P10*O10)+Q10>1000,IF($L$3<100,(P10*O10)+Q10,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L10*9550/K10,\"-\")","v":"-"},{"$f":"(K10*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"($L$2*0.0734971074173716*R10/9550)","v":0}]
[null,null,"B",{"$f":"E11/1450","v":7.1034482758620694E-4},1.03,{"$f":"D11*960","v":0.68193103448275871},{"$f":"D11*730","v":0.51855172413793105},0,{"$f":"$H$11*1000","v":0},{"$f":"$I$11/60","v":0},{"$f":"$J$11/$D$11","v":0},{"$f":"($L$2*0.0460581873148862*K11/9550)","v":0},{"$f":"IF(K11>10,IF((P11*O11)+Q11>1000,IF($L$3<100,(P11*O11)+Q11,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L11*9550/K11,\"-\")","v":"-"},{"$f":"(K11*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"($L$2*0.0460581873148862*R11/9550)","v":0}]
[null,null,"G",{"$f":"E12/1450","v":4.3448275862068968E-4},0.63,{"$f":"D12*960","v":0.4171034482758621},{"$f":"D12*730","v":0.31717241379310346},0,{"$f":"$H$12*1000","v":0},{"$f":"$I$12/60","v":0},{"$f":"$J$12/$D$12","v":0},{"$f":"($L$2*0.0333186886958751*K12/9550)","v":0},{"$f":"IF(K12>10,IF((P12*O12)+Q12>1000,IF($L$3<100,(P12*O12)+Q12,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L12*9550/K12,\"-\")","v":"-"},{"$f":"(K12*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"($L$2*0.0333186886958751*R12/9550)","v":0}]
[]
[null,"G03 / G13","X",{"$f":"E14/1450","v":6.4137931034482761E-3},9.3000000000000007,{"$f":"D14*960","v":6.1572413793103449},{"$f":"D14*730","v":4.6820689655172414},0,{"$f":"$H$14*1000","v":0},{"$f":"$I$14/60","v":0},{"$f":"$J$14/$D$14","v":0},{"$f":"(J14*$L$2/511)+(6*K14/84428)","v":0},{"$f":"IF(K14>10,IF((P14*O14)+Q14>1000,IF($L$3<100,(P14*O14)+Q14,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L14*9550/K14,\"-\")","v":"-"},{"$f":"(K14*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.0331950207468878,6159.7510373443984,null,{"$f":"(N14*$L$2/511)+(6*R14/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"E",{"$f":"E15/1450","v":4.6896551724137934E-3},6.8,{"$f":"D15*960","v":4.5020689655172417},{"$f":"D15*730","v":3.4234482758620692},0,{"$f":"$H$15*1000","v":0},{"$f":"$I$15/60","v":0},{"$f":"$J$15/$D$15","v":0},{"$f":"(J15*$L$2/511)+(6*K15/84428)","v":0},{"$f":"IF(K15>10,IF((P15*O15)+Q15>1000,IF($L$3<100,(P15*O15)+Q15,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L15*9550/K15,\"-\")","v":"-"},{"$f":"(K15*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.0331950207468878,6159.7510373443984,null,{"$f":"(N15*$L$2/511)+(6*R15/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"S",{"$f":"E16/1450","v":3.862068965517241E-3},5.6,{"$f":"D16*960","v":3.7075862068965515},{"$f":"D16*730","v":2.8193103448275858},0,{"$f":"$H$16*1000","v":0},{"$f":"$I$16/60","v":0},{"$f":"$J$16/$D$16","v":0},{"$f":"(J16*$L$2/511)+(6*K16/84428)","v":0},{"$f":"IF(K16>10,IF((P16*O16)+Q16>1000,IF($L$3<100,(P16*O16)+Q16,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L16*9550/K16,\"-\")","v":"-"},{"$f":"(K16*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.0331950207468878,6159.7510373443984,null,{"$f":"(N16*$L$2/511)+(6*R16/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"B",{"$f":"E17/1450","v":2.413793103448276E-3},3.5,{"$f":"D17*960","v":2.317241379310345},{"$f":"D17*730","v":1.7620689655172415},0,{"$f":"$H$17*1000","v":0},{"$f":"$I$17/60","v":0},{"$f":"$J$17/$D$17","v":0},{"$f":"(J17*$L$2/511)+(6*K17/84428)","v":0},{"$f":"IF(K17>10,IF((P17*O17)+Q17>1000,IF($L$3<100,(P17*O17)+Q17,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L17*9550/K17,\"-\")","v":"-"},{"$f":"(K17*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.0331950207468878,6159.7510373443984,null,{"$f":"(N17*$L$2/511)+(6*R17/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"G",{"$f":"E18/1450","v":1.0344827586206897E-3},1.5,{"$f":"D18*960","v":0.99310344827586206},{"$f":"D18*730","v":0.75517241379310351},0,{"$f":"$H$18*1000","v":0},{"$f":"$I$18/60","v":0},{"$f":"$J$18/$D$18","v":0},{"$f":"(J18*$L$2/511)+(6*K18/84428)","v":0},{"$f":"IF(K18>10,IF((P18*O18)+Q18>1000,IF($L$3<100,(P18*O18)+Q18,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L18*9550/K18,\"-\")","v":"-"},{"$f":"(K18*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.0331950207468878,6159.7510373443984,null,{"$f":"(N18*$L$2/511)+(6*R18/84428)","v":{"$error":"#VALUE!"}}]
[]
[null,"G04","X",6.2857E-3,{"$f":"D20*1450","v":9.1142649999999996},{"$f":"D20*960","v":6.0342719999999996},{"$f":"D20*730","v":4.5885610000000003},0,{"$f":"$H$20*1000","v":0},{"$f":"$I$20/60","v":0},{"$f":"$J$20/$D$20","v":0},{"$f":"(6*K20/84428)+(J20*L$2)/(511-((L$2-35)/4))","v":0},{"$f":"IF(K20>10,IF((P20*O20)+Q20>1000,IF($L$3<100,(P20*O20)+Q20,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L20*9550/K20,\"-\")","v":"-"},{"$f":"(K20*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-0.97213989330171902,6133.3728512151747,null,{"$f":"(6*R20/84428)+(N20*S$2)/(511-((S$2-35)/4))","v":{"$error":"#VALUE!"}}]
[null,"(Flows at 170 bar)","E",4.5710000000000004E-3,{"$f":"D21*1450","v":6.6279500000000002},{"$f":"D21*960","v":4.3881600000000001},{"$f":"D21*730","v":3.3368300000000004},0,{"$f":"$H$21*1000","v":0},{"$f":"$I$21/60","v":0},{"$f":"$J$21/$D$21","v":0},{"$f":"(6*K21/84428)+(J21*L$2)/(511-((L$2-35)/4))","v":0},{"$f":"IF(K21>10,IF((P21*O21)+Q21>1000,IF($L$3<100,(P21*O21)+Q21,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L21*9550/K21,\"-\")","v":"-"},{"$f":"(K21*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-0.97213989330171902,6133.3728512151747,null,{"$f":"(6*R21/84428)+(N21*S$2)/(511-((S$2-35)/4))","v":{"$error":"#VALUE!"}}]
[null,null,"S",3.4857E-3,{"$f":"D22*1450","v":5.054265},{"$f":"D22*960","v":3.3462719999999999},{"$f":"D22*730","v":2.5445609999999999},0,{"$f":"$H$22*1000","v":0},{"$f":"$I$22/60","v":0},{"$f":"$J$22/$D$22","v":0},{"$f":"(6*K22/84428)+(J22*L$2)/(511-((L$2-35)/4))","v":0},{"$f":"IF(K22>10,IF((P22*O22)+Q22>1000,IF($L$3<100,(P22*O22)+Q22,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L22*9550/K22,\"-\")","v":"-"},{"$f":"(K22*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-0.97213989330171902,6133.3728512151747,null,{"$f":"(6*R22/84428)+(N22*S$2)/(511-((S$2-35)/4))","v":{"$error":"#VALUE!"}}]
[]
[null,"G10 / G12","X",2.1100000000000001E-2,{"$f":"D24*1450","v":30.595000000000002},{"$f":"D24*960","v":20.256},{"$f":"D24*730","v":15.403},0,{"$f":"$H$24*1000","v":0},{"$f":"$I$24/60","v":0},{"$f":"$J$24/$D$24","v":0},{"$f":"(J24*$L$2/511)+(15*K24/84428)","v":0},{"$f":"IF(K24>10,IF((P24*O24)+Q24>1000,IF($L$3<100,(P24*O24)+Q24,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L24*9550/K24,\"-\")","v":"-"},{"$f":"(K24*$L$2*14.5*IF($L$3<35,1,0.927924*EXP(0.009267*$L$3)))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"(N24*$L$2/511)+(15*R24/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"E",1.9099999999999999E-2,{"$f":"D25*1450","v":27.694999999999997},{"$f":"D25*960","v":18.335999999999999},{"$f":"D25*730","v":13.943},0,{"$f":"$H$25*1000","v":0},{"$f":"$I$25/60","v":0},{"$f":"$J$25/$D$25","v":0},{"$f":"(J25*$L$2/511)+(15*K25/84428)","v":0},{"$f":"IF(K25>10,IF((P25*O25)+Q25>1000,IF($L$3<100,(P25*O25)+Q25,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L25*9550/K25,\"-\")","v":"-"},{"$f":"(K25*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"(N25*$L$2/511)+(15*R25/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"S",{"$f":"18.8/1450","v":1.2965517241379312E-2},18.8,{"$f":"D26*960","v":12.446896551724139},{"$f":"D26*730","v":9.4648275862068978},0,{"$f":"$H$26*1000","v":0},{"$f":"$I$26/60","v":0},{"$f":"$J$26/$D$26","v":0},{"$f":"(J26*$L$2/511)+(15*K26/84428)","v":0},{"$f":"IF(K26>10,IF((P26*O26)+Q26>1000,IF($L$3<100,(P26*O26)+Q26,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L26*9550/K26,\"-\")","v":"-"},{"$f":"(K26*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"(N26*$L$2/511)+(15*R26/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"I",{"$f":"12.5/1450","v":8.6206896551724137E-3},12.5,{"$f":"D27*960","v":8.2758620689655178},{"$f":"D27*730","v":6.2931034482758621},0,{"$f":"$H$27*1000","v":0},{"$f":"$I$27/60","v":0},{"$f":"$J$27/$D$27","v":0},{"$f":"(J27*$L$2/511)+(15*K27/84428)","v":0},{"$f":"IF(K27>10,IF((P27*O27)+Q27>1000,IF($L$3<100,(P27*O27)+Q27,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L27*9550/K27,\"-\")","v":"-"},{"$f":"(K27*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.594776748104465,6489.4692502106154,null,{"$f":"(N27*$L$2/511)+(15*R27/84428)","v":{"$error":"#VALUE!"}}]
[]
[null,"G15 / G17","X",3.3110000000000001E-2,{"$f":"1450*D29","v":48.009500000000003},{"$f":"D29*960","v":31.785600000000002},{"$f":"D29*730","v":24.170300000000001},0,{"$f":"$H$29*1000","v":0},{"$f":"$I$29/60","v":0},{"$f":"$J$29/$D$29","v":0},{"$f":"(80*K29/84428)+(J29*$L$2)/(511-(($L$2-35)/4))","v":0},{"$f":"IF(K29>10,IF((P29*O29)+Q29>1000,IF($L$3<100,(P29*O29)+Q29,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L29*9550/K29,\"-\")","v":"-"},{"$f":"(K29*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.309337134711333,6974.3406985032079,null,{"$f":"(80*R29/84428)+(N29*$L$2)/(511-(($L$2-35)/4))","v":{"$error":"#VALUE!"}}]
[null,"@138 bar","E",0.03,{"$f":"1450*D30","v":43.5},{"$f":"D30*960","v":28.799999999999997},{"$f":"D30*730","v":21.9},0,{"$f":"$H$30*1000","v":0},{"$f":"$I$30/60","v":0},{"$f":"$J$30/$D$30","v":0},{"$f":"(80*K30/84428)+(J30*$L$2)/(511-(($L$2-35)/4))","v":0},{"$f":"IF(K30>10,IF((P30*O30)+Q30>1000,IF($L$3<100,(P30*O30)+Q30,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L30*9550/K30,\"-\")","v":"-"},{"$f":"(K30*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.309337134711333,6974.3406985032079,null,{"$f":"(80*R30/84428)+(N30*$L$2)/(511-(($L$2-35)/4))","v":{"$error":"#VALUE!"}}]
[]
[null,"G25","X",7.2301369199999993E-2,"N/A",69,{"$f":"D32*730","v":52.779999515999997},0,{"$f":"$H$32*1000","v":0},{"$f":"$I$32/60","v":0},{"$f":"$J$32/$D$32","v":0},{"$f":"(J32*$L$2/511)+(50*K32/84428)","v":0},{"$f":"IF(K32>10,IF((P32*O32)+Q32>1000,IF($L$3<100,(P32*O32)+Q32,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L32*9550/K32,\"-\")","v":"-"},{"$f":"(K32*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-3.5,5825,null,{"$f":"(N32*$L$2/511)+(50*R32/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"E",6.6799999999999998E-2,null,63,{"$f":"D33*730","v":48.763999999999996},0,{"$f":"$H$33*1000","v":0},{"$f":"$I$33/60","v":0},{"$f":"$J$33/$D$33","v":0},{"$f":"(J33*$L$2/511)+(50*K33/84428)","v":0},{"$f":"IF(K33>10,IF((P33*O33)+Q33>1000,IF($L$3<100,(P33*O33)+Q33,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L33*9550/K33,\"-\")","v":"-"},{"$f":"(K33*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-3.5,5825,null,{"$f":"(N33*$L$2/511)+(50*R33/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"S",5.3499999999999999E-2,null,50,{"$f":"D34*730","v":39.055},0,{"$f":"$H$34*1000","v":0},{"$f":"$I$34/60","v":0},{"$f":"$J$34/$D$34","v":0},{"$f":"(J34*$L$2/511)+(50*K34/84428)","v":0},{"$f":"IF(K34>10,IF((P34*O34)+Q34>1000,IF($L$3<100,(P34*O34)+Q34,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L34*9550/K34,\"-\")","v":"-"},{"$f":"(K34*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-3.5,5825,null,{"$f":"(N34*$L$2/511)+(50*R34/84428)","v":{"$error":"#VALUE!"}}]
[null,null,"I",4.1000000000000002E-2,null,36,{"$f":"D35*730","v":29.93},0,{"$f":"$H$35*1000","v":0},{"$f":"$I$35/60","v":0},{"$f":"$J$35/$D$35","v":0},{"$f":"(J35*$L$2/511)+(50*K35/84428)","v":0},{"$f":"IF(K35>10,IF((P35*O35)+Q35>1000,IF($L$3<100,(P35*O35)+Q35,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L35*9550/K35,\"-\")","v":"-"},{"$f":"(K35*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-3.5,5825,null,{"$f":"(N35*$L$2/511)+(50*R35/84428)","v":{"$error":"#VALUE!"}}]
[]
[null,"G35",null,null,"@1050 max"]
[null,null,"X",{"$f":"F38/960","v":0.13229166666666667},140,127,{"$f":"D38*730","v":96.572916666666671},0,{"$f":"$H$38*1000","v":0},{"$f":"$I$38/60","v":0},{"$f":"$J$38/$D$38","v":0},{"$f":"(J38*$L$2/511)+(100*K38/84428)","v":0},{"$f":"IF(K38>10,IF((P38*O38)+Q38>1000,IF($L$3<100,(P38*O38)+Q38,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L38*9550/K38,\"-\")","v":"-"},{"$f":"(K38*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.9452771000348554,5945.974207040781,null,{"$f":"(N38*$L$2/511)+(100*R38/84428)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"@1150 max"]
[null,null,"E",{"$f":"F40/960","v":0.11458333333333333},132,110,{"$f":"D40*730","v":83.645833333333329},0,{"$f":"$H$40*1000","v":0},{"$f":"$I$40/60","v":0},{"$f":"$J$40/$D$40","v":0},{"$f":"(J40*$L$2/511)+(100*K40/84428)","v":0},{"$f":"IF(K40>10,IF((P40*O40)+Q40>1000,IF($L$3<100,(P40*O40)+Q40,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L40*9550/K40,\"-\")","v":"-"},{"$f":"(K40*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},-2.9452771000348554,5945.974207040781,null,{"$f":"(N40*$L$2/511)+(100*R40/84428)","v":{"$error":"#VALUE!"}}]
[]
[null,"G66","X",0.248,"1000 max",238.08,181.04,0,{"$f":"$H$42*1000","v":0},{"$f":"$I$42/60","v":0},{"$f":"$J$42/$D$42","v":0},{"$f":"(J42*$L$2/511)+(100*K42/84428)","v":0},{"$f":"IF(K42>10,IF((P42*O42)+Q42>1000,IF($L$3<100,(P42*O42)+Q42,\"Use Cooler\"),\"Use Cooler\"),NA())","v":{"$error":"#N/A"}},{"$f":"IFERROR(L42*9550/K42,\"-\")","v":"-"},{"$f":"(K42*$L$2*14.5*IF($L$3<35,1,IF($L$3<60,1.3,IF($L$3<85,1.6,IF($L$3<105,2,2.5)))))/1000","v":0},{"$f":"NA()","v":{"$error":"#N/A"}},null,null,{"$f":"(N42*$L$2/511)+(100*R42/84428)","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,"@ 450 rpm","@ 45 rpm                  (Minimum Speed)","Minimum speed at input discharge pressure RPM"]
["Low Pressure","T100E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pick the row which is closest to the operating discharge pressure to enter flow rate."]
[null,"(35 Bar)",null,0.83499999999999996,{"$f":"D46*450","v":375.75},{"$f":"D46*200","v":167},{"$f":"$L$2/(103/45)","v":4.3689320388349513},{"$f":"$I$46/1000","v":0},{"$f":"$J$46*60","v":0},null,{"$f":"$J$46/$D$46","v":0},{"$f":"J46*$L$2/511","v":0},2000,{"$f":"IFERROR(L46*9550/K46,\"-\")","v":"-"},null,null,null,null,{"$f":"N46*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(69 Bar)",null,0.82499999999999996,{"$f":"D47*450","v":371.25},{"$f":"D47*200","v":165},null,{"$f":"$I$47/1000","v":0},{"$f":"$J$47*60","v":0},null,{"$f":"$J$47/$D$47","v":0},{"$f":"J47*$L$2/511","v":0},2000,{"$f":"IFERROR(L47*9550/K47,\"-\")","v":"-"},null,null,null,null,{"$f":"N47*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(103 Bar)",null,0.81399999999999995,{"$f":"D48*450","v":366.29999999999995},{"$f":"D48*200","v":162.79999999999998},null,{"$f":"$I$48/1000","v":0},{"$f":"$J$48*60","v":0},null,{"$f":"$J$48/$D$48","v":0},{"$f":"J48*$L$2/511","v":0},2000,{"$f":"IFERROR(L48*9550/K48,\"-\")","v":"-"},null,null,null,null,{"$f":"N48*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,"T100F"]
[null,"(35 Bar)",null,null,null,null,null,{"$f":"$I$51/1000","v":0},{"$f":"$J$51*60","v":0},null,{"$f":"$J$51/$D$51","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(L51*9550/K51,\"-\")","v":"-"}]
[null,"(69 Bar)",null,null,null,null,null,{"$f":"$I$52/1000","v":0},{"$f":"$J$52*60","v":0},null,{"$f":"$J$52/$D$52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(L52*9550/K52,\"-\")","v":"-"}]
[null,"(127 Bar)",null,{"$f":"290/450","v":0.64444444444444449},{"$f":"D53*450","v":290},{"$f":"D53*200","v":128.88888888888889},{"$f":"$L$2/(127/45)","v":3.5433070866141732},{"$f":"$I$53/1000","v":0},{"$f":"$J$53*60","v":0},null,{"$f":"$J$53/$D$53","v":0},{"$f":"J53*$L$2/511","v":0},2000,{"$f":"IFERROR(L53*9550/K53,\"-\")","v":"-"}]
[]
[null,"T100H"]
[null,"(35 Bar)",null,null,null,null,null,{"$f":"$I$56/1000","v":0},{"$f":"$J$56*60","v":0},null,{"$f":"$J$56/$D$56","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(L56*9550/K56,\"-\")","v":"-"}]
[null,"(69 Bar)",null,null,null,null,null,{"$f":"$I$57/1000","v":0},{"$f":"$J$57*60","v":0},null,{"$f":"$J$57/$D$57","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(L57*9550/K57,\"-\")","v":"-"}]
[null,"(144 Bar)",null,{"$f":"258/450","v":0.57333333333333336},{"$f":"D58*450","v":258},{"$f":"D58*200","v":114.66666666666667},{"$f":"$L$2/(144/45)","v":3.125},0,{"$f":"$H$58*1000","v":0},{"$f":"$I$58/60","v":0},{"$f":"$J$58/$D$58","v":0},{"$f":"J58*$L$2/511","v":0},2000,{"$f":"IFERROR(L58*9550/K58,\"-\")","v":"-"}]
[]
["Med Pressure","T100K"]
[null,"(207 bar)",null,{"$f":"E61/450","v":0.38444444444444442},173,76.888888888888886,{"$f":"$L$2/(207/45)","v":2.1739130434782612},{"$f":"$I$61/1000","v":0},{"$f":"$J$61*60","v":0},null,{"$f":"$J$61/$D$61","v":0},{"$f":"J61*$L$2/511","v":0},2000,{"$f":"IFERROR(L61*9550/K61,\"-\")","v":"-"},null,null,null,null,{"$f":"N61*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(103 bar)",null,{"$f":"E62/450","v":0.39777777777777779},179,80,null,{"$f":"$I$62/1000","v":0},{"$f":"$J$62*60","v":0},null,{"$f":"$J$62/$D$62","v":0},{"$f":"J62*$L$2/511","v":0},2000,{"$f":"IFERROR(L62*9550/K62,\"-\")","v":"-"},null,null,null,null,{"$f":"N62*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(35 bar)",null,{"$f":"E63/450","v":0.40888888888888891},184,82,null,{"$f":"$I$63/1000","v":0},{"$f":"$J$63*60","v":0},null,{"$f":"$J$63/$D$63","v":0},{"$f":"J63*$L$2/511","v":0},2000,{"$f":"IFERROR(L63*9550/K63,\"-\")","v":"-"},null,null,null,null,{"$f":"N63*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,"T100M"]
[null,"(245 bar)",null,{"$f":"E66/450","v":0.32},144,{"$f":"E66*200/450","v":64},{"$f":"$L$2/(245/45)","v":1.8367346938775511},{"$f":"$I$66/1000","v":0},{"$f":"$J$66*60","v":0},null,{"$f":"$J$66/$D$66","v":0},{"$f":"J66*$L$2/511","v":0},2000,{"$f":"IFERROR(L66*9550/K66,\"-\")","v":"-"},null,null,null,null,{"$f":"N66*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
["High Pressure","T100S"]
[null,"(35 Bar)",null,0.249,110,49,{"$f":"$L$2/(345/45)","v":1.3043478260869565},{"$f":"$I$69/1000","v":0},{"$f":"$J$69*60","v":0},null,{"$f":"$J$69/$D$69","v":0},{"$f":"J69*$L$2/511","v":0},2000,{"$f":"IFERROR(L69*9550/K69,\"-\")","v":"-"},null,null,null,null,{"$f":"N69*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(172 Bar)",null,0.23699999999999999,104,47,null,{"$f":"$I$70/1000","v":0},{"$f":"$J$70*60","v":0},null,{"$f":"$J$70/$D$70","v":0},{"$f":"J70*$L$2/511","v":0},2000,{"$f":"IFERROR(L70*9550/K70,\"-\")","v":"-"},null,null,null,null,{"$f":"N70*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(345 Bar)",null,0.222,98,43,null,{"$f":"$I$71/1000","v":0},{"$f":"$J$71*60","v":0},null,{"$f":"$J$71/$D$71","v":0},{"$f":"J71*$L$2/511","v":0},2000,{"$f":"IFERROR(L71*9550/K71,\"-\")","v":"-"},null,null,null,null,{"$f":"N71*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,"@ 450 rpm","@ 45 rpm                  (Minimum Speed)","Minimum speed at input discharge pressure RPM"]
["Low Pressure","Q155E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pick the row which is closest to the operating discharge pressure to enter flow rate."]
[null,"(35 Bar)",null,1.3540000000000001,{"$f":"D75*450","v":609.30000000000007},{"$f":"D75*200","v":270.8},{"$f":"$L$2/(103/45)","v":4.3689320388349513},0,{"$f":"$H$75*1000","v":0},{"$f":"$I$75/60","v":0},{"$f":"$J$75/$D$75","v":0},{"$f":"J75*$L$2/511","v":0},2000,{"$f":"IFERROR(L75*9550/K75,\"-\")","v":"-"},null,null,null,null,{"$f":"N75*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(69 Bar)",null,1.3380000000000001,{"$f":"D76*450","v":602.1},{"$f":"D76*200","v":267.60000000000002},null,{"$f":"$I$76/1000","v":0},{"$f":"$J$76*60","v":0},null,{"$f":"$J$76/$D$76","v":0},{"$f":"J76*$L$2/511","v":0},2000,{"$f":"IFERROR(L76*9550/K76,\"-\")","v":"-"},null,null,null,null,{"$f":"N76*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(103 Bar)",null,1.323,{"$f":"D77*450","v":595.35},{"$f":"D77*200","v":264.59999999999997},null,0,{"$f":"$H$77*1000","v":0},{"$f":"$I$77/60","v":0},{"$f":"$J$77/$D$77","v":0},{"$f":"J77*$L$2/511","v":0},2000,{"$f":"IFERROR(L77*9550/K77,\"-\")","v":"-"},null,null,null,null,{"$f":"N77*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,"Q155F"]
[null,"(35 Bar)",null,1.1020000000000001,{"$f":"D80*450","v":495.90000000000003},{"$f":"D80*200","v":220.4},{"$f":"$L$2/(127/45)","v":3.5433070866141732},{"$f":"$I$80/1000","v":0},{"$f":"$J$80*60","v":0},null,{"$f":"$J$80/$D$80","v":0},{"$f":"J80*$L$2/511","v":0},2000,{"$f":"IFERROR(L80*9550/K80,\"-\")","v":"-"},null,null,null,null,{"$f":"N80*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(69 Bar)",null,1.085,{"$f":"D81*450","v":488.25},{"$f":"D81*200","v":217},null,{"$f":"$I$81/1000","v":0},{"$f":"$J$81*60","v":0},null,{"$f":"$J$81/$D$81","v":0},{"$f":"J81*$L$2/511","v":0},2000,{"$f":"IFERROR(L81*9550/K81,\"-\")","v":"-"},null,null,null,null,{"$f":"N81*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(127 Bar)",null,1.0680000000000001,{"$f":"D82*450","v":480.6},{"$f":"D82*200","v":213.60000000000002},null,{"$f":"$I$82/1000","v":0},{"$f":"$J$82*60","v":0},null,{"$f":"$J$82/$D$82","v":0},{"$f":"J82*$L$2/511","v":0},2000,{"$f":"IFERROR(L82*9550/K82,\"-\")","v":"-"},null,null,null,null,{"$f":"N82*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[]
[null,"Q155H",null,0.96699999999999997,{"$f":"D85*450","v":435.15},{"$f":"D85*200","v":193.4},{"$f":"$L$2/(144/45)","v":3.125},{"$f":"$I$85/1000","v":0},{"$f":"$J$85*60","v":0},null,{"$f":"$J$85/$D$85","v":0},{"$f":"J85*$L$2/511","v":0},2000,{"$f":"IFERROR(L85*9550/K85,\"-\")","v":"-"},null,null,null,null,{"$f":"N85*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(69 Bar)",null,0.95099999999999996,{"$f":"D86*450","v":427.95},{"$f":"D86*200","v":190.2},null,{"$f":"$I$86/1000","v":0},{"$f":"$J$86*60","v":0},null,{"$f":"$J$86/$D$86","v":0},{"$f":"J86*$L$2/511","v":0},2000,{"$f":"IFERROR(L86*9550/K86,\"-\")","v":"-"},null,null,null,null,{"$f":"N86*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(144 Bar)",null,0.93600000000000005,{"$f":"D87*450","v":421.20000000000005},{"$f":"D87*200","v":187.20000000000002},null,0,{"$f":"$H$87*1000","v":0},{"$f":"$I$87/60","v":0},{"$f":"$J$87/$D$87","v":0},{"$f":"J87*$L$2/511","v":0},2000,{"$f":"IFERROR(L87*9550/K87,\"-\")","v":"-"},null,null,null,null,{"$f":"N87*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
["Med Pressure","Q155K"]
[null,"(35 Bar)",null,0.7,173,76.888888888888886,{"$f":"$L$2/(207/45)","v":2.1739130434782612},{"$f":"$I$90/1000","v":0},{"$f":"$J$90*60","v":0},null,{"$f":"$J$90/$D$90","v":0},{"$f":"J90*$L$2/511","v":0},2000,{"$f":"IFERROR(L90*9550/K90,\"-\")","v":"-"},null,null,null,null,{"$f":"N90*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(103 bar)",null,0.68500000000000005,179,80,null,{"$f":"$I$91/1000","v":0},{"$f":"$J$91*60","v":0},null,{"$f":"$J$91/$D$91","v":0},{"$f":"J91*$L$2/511","v":0},2000,{"$f":"IFERROR(L91*9550/K91,\"-\")","v":"-"},null,null,null,null,{"$f":"N91*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(207 bar)",null,0.65400000000000003,184,82,null,0,{"$f":"$H$92*1000","v":0},{"$f":"$I$92/60","v":0},{"$f":"$J$92/$D$92","v":0},{"$f":"J92*$L$2/511","v":0},2000,{"$f":"IFERROR(L92*9550/K92,\"-\")","v":"-"},null,null,null,null,{"$f":"N92*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,"Q155M"]
[null,"(241 bar)",null,0.54700000000000004,{"$f":"D95*450","v":246.15},{"$f":"E95*200/450","v":109.4},{"$f":"$L$2/(241/45)","v":1.8672199170124482},{"$f":"$I$95/1000","v":0},{"$f":"$J$95*60","v":0},null,{"$f":"$J$95/$D$95","v":0},{"$f":"J95*$L$2/511","v":0},2000,{"$f":"IFERROR(L95*9550/K95,\"-\")","v":"-"},null,null,null,null,{"$f":"N95*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"@ 400 rpm","@ 40rpm                  (Minimum Speed)","Minimum speed at input discharge pressure RPM"]
["Med Pressure","T200K",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pick the row which is closest to the operating discharge pressure to enter flow rate."]
[null,"(207 bar)",null,0.91400000000000003,{"$f":"D98*400","v":365.6},{"$f":"E98/10","v":36.56},{"$f":"$L$2/(207/40)","v":1.9323671497584543},{"$f":"$I$61/1000","v":0},{"$f":"$J$61*60","v":0},null,{"$f":"$J$61/$D$61","v":0},{"$f":"J98*$L$2/511","v":0},2000,{"$f":"IFERROR(L98*9550/K98,\"-\")","v":"-"},null,null,null,null,{"$f":"N98*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(103 bar)",null,0.94899999999999995,{"$f":"D99*400","v":379.59999999999997},{"$f":"E99/10","v":37.959999999999994},null,{"$f":"$I$62/1000","v":0},{"$f":"$J$62*60","v":0},null,{"$f":"$J$62/$D$62","v":0},{"$f":"J99*$L$2/511","v":0},2000,{"$f":"IFERROR(L99*9550/K99,\"-\")","v":"-"},null,null,null,null,{"$f":"N99*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(35 bar)",null,0.96899999999999997,387.59999999999997,38.76,null,{"$f":"$I$63/1000","v":0},{"$f":"$J$63*60","v":0},null,{"$f":"$J$63/$D$63","v":0},{"$f":"J100*$L$2/511","v":0},2000,{"$f":"IFERROR(L100*9550/K100,\"-\")","v":"-"},null,null,null,null,{"$f":"N100*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,"T200M"]
[null,"(245 bar)",null,0.8,{"$f":"D103*400","v":320},{"$f":"E103/10","v":32},{"$f":"$L$2/(245/40)","v":1.6326530612244898},{"$f":"$I$66/1000","v":0},{"$f":"$J$66*60","v":0},null,{"$f":"$J$66/$D$66","v":0},{"$f":"J103*$L$2/511","v":0},2000,{"$f":"IFERROR(L103*9550/K103,\"-\")","v":"-"},null,null,null,null,{"$f":"N103*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
["High Pressure","T200P"]
[null,"(35 Bar)",null,0.76800000000000002,{"$f":"D106*400","v":307.2},{"$f":"E106/10","v":30.72},{"$f":"$L$2/(276/40)","v":1.4492753623188406},{"$f":"$I$69/1000","v":0},{"$f":"$H$106*1000","v":0},{"$f":"$I$106/60","v":0},{"$f":"$J$106/$D$106","v":0},{"$f":"J106*$L$2/511","v":0},2000,{"$f":"IFERROR(L106*9550/K106,\"-\")","v":"-"},null,null,null,null,{"$f":"N106*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(138 Bar)",null,0.749,299.60000000000002,29.96,null,{"$f":"$I$70/1000","v":0},{"$f":"$J$70*60","v":0},null,{"$f":"$J$70/$D$70","v":0},{"$f":"J107*$L$2/511","v":0},2000,{"$f":"IFERROR(L107*9550/K107,\"-\")","v":"-"},null,null,null,null,{"$f":"N107*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(276 Bar)",null,0.71199999999999997,284.8,28.48,null,{"$f":"$I$71/1000","v":0},{"$f":"$J$71*60","v":0},null,{"$f":"$J$71/$D$71","v":0},{"$f":"J108*$L$2/511","v":0},2000,{"$f":"IFERROR(L108*9550/K108,\"-\")","v":"-"},null,null,null,null,{"$f":"N108*$L$2/511","v":{"$error":"#VALUE!"}}]
[]
[null,"T200Q"]
[null,"(35 Bar)",null,0.67400000000000004,{"$f":"D111*400","v":269.60000000000002},{"$f":"E111/10","v":26.96},{"$f":"$L$2/(310/40)","v":1.2903225806451613},0,{"$f":"$H$111*1000","v":0},{"$f":"$I$111/60","v":0},{"$f":"$J$111/$D$111","v":0},{"$f":"J111*$L$2/511","v":0},2000,{"$f":"IFERROR(L111*9550/K111,\"-\")","v":"-"},null,null,null,null,{"$f":"N111*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(155 Bar)",null,0.65500000000000003,262,26.2,null,0,{"$f":"$H$112*1000","v":0},{"$f":"$I$112/60","v":0},{"$f":"$J$112/$D$112","v":0},{"$f":"J112*$L$2/511","v":0},2000,{"$f":"IFERROR(L112*9550/K112,\"-\")","v":"-"},null,null,null,null,{"$f":"N112*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"(310 Bar)",null,0.625,250,25,null,0,{"$f":"$H$113*1000","v":0},{"$f":"$I$113/60","v":0},{"$f":"$J$113/$D$113","v":0},{"$f":"J113*$L$2/511","v":0},2000,{"$f":"IFERROR(L113*9550/K113,\"-\")","v":"-"},null,null,null,null,{"$f":"N113*$L$2/511","v":{"$error":"#VALUE!"}}]
[null,"Actual flows may vary by +/- 5%"]

{"sheet":"Oil Change Intervals","index":1,"n_rows":21,"n_cols":22,"rows_kept":21,"cut":false,"hidden":true,"merged":[]}
[]
[null,"G20","Series",null,"G15","Series",null,"G03","Series",null,"G25","Series",null,"G04","Series",null,"G35","Series",null,"G10","Series"]
[null,950,4000,null,1200,4000,null,1050,4000,null,550,4000,null,2150,4000,null,650,4000,null,950,4000]
[null,1350,3000,null,1900,3000,null,1550,3000,null,750,3000,null,3250,3000,null,1000,3000,null,1350,3000]
[null,1750,2000,null,2200,2000,null,2100,2000,null,1150,2000,null,4350,2000,null,1380,2000,null,1750,2000]
[null,2100,1000,null,2450,1000,null,2500,1000,null,1350,1000,null,5200,1000,null,1650,1000,null,2100,1000]
[null,"Slope",{"$f":"SLOPE(C3:C6,B3:B6)","v":-2.594776748104465},null,"Slope",{"$f":"SLOPE(F3:F6,E3:E6)","v":-2.309337134711333},null,"Slope",{"$f":"SLOPE(I3:I6,H3:H6)","v":-2.0331950207468878},null,"Slope",{"$f":"SLOPE(L3:L6,K3:K6)","v":-3.5},null,"Slope",{"$f":"SLOPE(O3:O6,N3:N6)","v":-0.97213989330171902},null,"Slope",{"$f":"SLOPE(R3:R6,Q3:Q6)","v":-2.9452771000348554},null,"Slope",{"$f":"SLOPE(U3:U6,T3:T6)","v":-2.594776748104465},{"$f":"INTERCEPT(U3:U6,T3:T6)","v":6489.4692502106154}]
[null,"Intercept",{"$f":"INTERCEPT(C3:C6,B3:B6)","v":6489.4692502106154},null,"Intercept",{"$f":"INTERCEPT(F3:F6,E3:E6)","v":6974.3406985032079},null,"Intercept",{"$f":"INTERCEPT(I3:I6,H3:H6)","v":6159.7510373443984},null,"Intercept",{"$f":"INTERCEPT(L3:L6,K3:K6)","v":5825},null,"Intercept",{"$f":"INTERCEPT(O3:O6,N3:N6)","v":6133.3728512151747},null,"Intercept",{"$f":"INTERCEPT(R3:R6,Q3:Q6)","v":5945.974207040781},null,"Intercept"]
[]
[]
[]
[]
[]
[]
[]
[null,"Temperature","Factor"]
[]
[null,35,1.3]
[null,60,1.6]
[null,85,2]
[null,105,2.5]

{"sheet":"T100 Oil Change","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Torque","index":3,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":true,"merged":[[6,6,6,7]]}
[]
[null,"Torque Calculation for Hydra-Cell pumps"]
[]
[null,null,null,"Using:",null,"Nm =","kW","X",9550]
[null,null,null,null,null,null,null,"r.p.m."]
[]
[null,"ENTER",">","kW:",null,1,"speed, r.p.m.:",null,500]
[]
[null,null,null,"Torque required =",null,null,{"$f":"F7*9550/I7","v":19.100000000000001},"Nm"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"KW = Nm*RPM/9550"]
[]
[null,null,null,null,null,null,"Torque",19.100000000000001,"Nm"]
[null,null,null,null,null,null,"RPM",500]
[null,null,null,null,null,null,"Power",{"$f":"H17*H18/9550","v":1},"kW"]

{"sheet":"MotorInverter Approx KW","index":4,"n_rows":10,"n_cols":3,"rows_kept":10,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,"Mains supply frequency f1 (Hz)",50]
[]
[null,"Requirred frequency for rpm f2 (Hz)",100]
[]
[null,"Power of motor at supply frenquency  P1 (KW)",1]
[]
[null,"Approx Power of motor at requirred RPM P2 (KW)",{"$f":"(POWER((C6/C4),2))*C8","v":4}]